1. My browser only send 1 GET message. The packet number is 58.
2. 61,62,63,64
3. Status code: #61:ACK; #62:PSH,ACK; #63: ACK; #64: ACK; the phrase: TCP segment of a reassembled PDU. 62 TCP previous segment not captured. 63 TCP Out-Of-Order. 64: TCP Out-of-order.
4. 4 Reassembled TCP segments(4861 bytes): #61(1460), #62(481), #63(1460), #64(1460).
5. My browser send 3 GET request. The address is 128.119.245.12
6. My browser download the two images in parallel. My browser initialize two TCP connection with the server to receive the files. (From port 58754 to 80. From port 58756 to 80).
7. Status: 401 phrase: Unauthorized
8. This Authorization header field: Authorization: Basic d2lyZXNoYXJrLXN0dWRlbnRzOm5ldHdvcms=\r\n, is inserted to the second GET message.